**Restriktioner ESDEC EVO**

2

Wind sensitivity

For both ClickFit EVO tile and Steelback, what is the maximum height to install it on? Steeldeck: 15 meters, Tile: 12 meters.

In general is EVO tile suitable with a maximum windload of 1350 n/m2.